**Fatality Assessment and Control Evaluation (FACE) Program**

**Forklift Operator Crushed Between Forklift Cage and**

**Mast while Loading Waste Paper into a Trailer ­**

**Massachusetts**

Massachusetts Case Report: 08­MA­019                      Release Date: March 16, 2010

**Summary**

On April 4, 2008 a 61­year­old male forklift/baler operator (victim) was fatally injured when he was

crushed between the cage and mast of the forklift he was operating. The victim was positioning a

pallet loaded with waste corrugated cardboard boxes on top of other stacked pallets inside a tractor

trailer. The pallet loaded on the forklift tines was lowered onto the stacked pallets inside the trailer,

but would not slide off the raised forklift tines. The victim exited the forklift operator’s area to assess

where the pallet was caught. While climbing up onto the exterior front section of the forklift and then

reaching up between the forklift cage and mast, the victim’s foot came in contact with and engaged

the forklift’s mast tilting control lever. The mast tilted back, crushing the victim between the mast and

forklift cage. The victim was found by a co­worker who placed a call for emergency medical services

(EMS). Co­workers then freed the victim from the forklift. The local fire department arrived within

minutes and started cardiopulmonary resuscitation (CPR). The victim was then transported to a local

hospital where he was pronounced dead. The Massachusetts FACE Program concluded that to

prevent similar occurrences in the future, employers should:

**Ensure that forklift operators never position themselves or any part of their bodies**

**between the forklift operator’s cage and the upright of the mast while the forklift is**

**running;**

**Ensure that standard operating procedures (SOP) are followed during forklift operation**

**and that SOPs include alternative procedures for non­routine tasks, such as inability to**

**lower the tines;**

**Ensure adequate light is provided in locations where forklifts are operated;**

**Ensure that all federal and state required trainings and licenses for forklift operators are**

**up to date; and**

**Routinely evaluate the effectiveness of health and safety programs and activities in the**

**workplace.**

Forklifts manufacturers should:

**Design forklifts so that operators cannot place any parts of their body in between the**

**cage and mast and unintentionally engage the mast controls.**

**Introduction**

On April 8, 2008, the Massachusetts FACE Program was notified by the Occupational Safety and

Health Administration (OSHA) through the 24­hour Occupational Fatality Hotline that on April 4,

2008, a 61­year­old male forklift operator had died when he was caught between the forklift’s mast

and cage. On May 13, 2008, the Massachusetts FACE Program Director and an investigator traveled

to the employer location and met with multiple company representatives to discuss the incident. The

OSHA fatality and catastrophe report, fire department report, death certificate, company information,

and the forklift information were reviewed during the course of the investigation.

The employer is an envelope manufacturer that was founded in the early 1950s and now has

locations throughout the United States. The Massachusetts location, where the incident occurred,

was established in 1971. This manufacturer employs approximately 4,000 workers nationwide, with

the incident location accounting for 185 employees. Of the 185 employees, 154 are paid hourly

wages and 31 receive salaries. The company has a five­day work week with three shifts per day. The

first shift, the shift during which the incident occurred, starts at 7:00 a.m. and ends at 3:00 p.m. The

victim’s job title was forklift/baler operator. There is only one forklift/baler operator working per shift.

The victim, an immigrant from Poland, had been employed by the company for 26 years. At the time

of the incident, there were approximately 65 employees on site within the manufacturing facility, not

including office employees.

The company has a written health and safety program and standard operating procedures (SOP) for

operating machines and completing tasks. Both the health and safety program and SOPs are

developed at the corporate level and modified for each facility. The company has a joint

**Massachusetts Case**

**Report**

[NIOSH FACE Home](http://www.cdc.gov/niosh/face/default.html)

[State­based Case Reports](http://www.cdc.gov/niosh/face/stateface.html)

[Massachusetts Case Reports](http://www2a.cdc.gov/NIOSH-FACE/state.asp?Category=0000&Category2=ALL&State=MA&Submit=Submit)

**On This Page...**

  • Summary

  • Introduction

  • Investigation

  • Cause of Death

  • Recommendations and

    Discussion

  • References

management­labor health and safety committee that meets monthly. The worker representatives are

selected by management, and serve varying terms on the committee. The company provides

employees health and safety training that is primarily on­the­job training with some classroom

exercises and safety videos. New employees are paired with more experienced employees as part

of their on­the­job training and are evaluated weekly by the shift supervisor to assess competencies.

It was reported that federally required forklift­specific training and certification process is renewed

every three years and includes classroom, video, and on­the­job training as well as employee

evaluation. At the time of the incident, the forklift certification for the victim had lapsed by

approximately two weeks. In addition, none of the forklift operators had the state required Hoisting

License. The victim was part of a collective bargaining unit.

**Back to Top**

**Investigation**

The company owns multiple fork trucks, including sit­down forklifts, standing forklifts, and walkers, but

the forklift involved in the incident was not owned by the company. This forklift was owned by one of

the company’s vendors, a waste paper company (Figure #1). The company has a contract with this

waste paper vendor which includes having a trailer located at the company’s loading dock and a sit

down forklift onsite to load the trailer. The vender’s forklift was used only by the envelope company

employees, including the victim. The forklift was used to collect waste paper throughout the facility.

Once collected, the waste paper was either baled or stacked onto wooden pallets and stored by the

loading dock area. The forklift was also used to load the paper bales and pallets into the vendor’s

trailer stationed at the loading dock. Once the trailer was full, the waste paper vendor traveled to the

company location, picked up the loaded trailer and dropped off an empty trailer.

The vendor’s forklift was a sit­down propane powered forklift. The forklift was manufactured in 1987

and has been located at the company since 2001 (Figure #1). The forklift is equipped with a cage

around the operator’s area and two lights attached to the two pillars that make up the front of the

cage. Three control levers are located to the right of the forklift’s steering wheel (Figure #2). These

levers are used to adjust the forklift tines and mast. The lever closest to the steering wheel raises and

lowers the tines. The middle lever, when pulled down, tilts the mast back towards the forklift’s cage,

which in turn angles the far end of the tines up. When the middle lever is pushed forward it tilts the

forklift mast forward away from the forklift cage and angles the far end of the tines back towards the

ground. The lever furthest to the right of the steering wheel shifts the tines from side to side.

On the day of the incident, the victim was working a normal work shift and started his work day at

7:00 a.m. At the time of the incident, approximately 9:40 a.m., the victim was loading flattened

corrugated boxes strapped to pallets into the waste paper tractor trailer located at the company’s

loading dock. This area of the loading dock was equipped with an adjustable light to be used when

trailers were being loaded (Figure #3). At the time of the incident the dock light was on, but it was

unclear if the dock light was working properly, potentially resulting in the trailer being dimly lit. In

addition, only one of the two forklift lights was functioning at the time of the incident.

The trailer, which was wide enough to be loaded with two rows of pallets stacked side by side, was

approximately one quarter full at the time of the incident. The pallets located on the right side of the

trailer were stacked up to the trailer’s roof. The pallet stack on the left side of the trailer had room for

more pallets. The victim used the forklift to pick up a pallet loaded with waste cardboard, which had

been stored next to the loading dock. The plastic strapping that secured the cardboard to the pallet

wound around the front and back sides of the pallet and cardboard, the straps running over the top

and through the bottom of the pallet (Figure #4). The victim transported the pallet on the forklift tines

into the trailer. He positioned the forklift close to the trailer’s left side to place the pallet on top of the

left stack.

The forklift’s tines were raised about six feet as the victim placed the pallet of corrugated cardboard

on top of the pallets already stacked on the left. Although the incident was not witnessed, evidence

indicates that the following sequence of events took place. After placing the raised pallet on top of

the other stacked pallets, the victim started to back the forklift. The strapping securing the cardboard

to the pallet became caught on a bolt on the forklift’s mast. After backing approximately two feet, the

pallet started to move back with the forklift. It appears that, at this point, the victim was unable to move

the load forward to reposition the pallet back on top of the stacked pallets, and that if he continued to

back the forklift, the loaded pallet potentially would have fallen off both the stacked pallets and the

forklift’s tines.

From this point forward it is unclear if the victim was trying to fix the problem or if he was attempting to

get a better look at why the pallet was hung up. While the forklift was running and the tines were still

raised approximately six feet, the victim engaged the forklift’s emergency brake and exited the forklift

operator’s area. Evidence indicates that the victim then climbed up onto the exterior of the forklift

between the forklift mast and the forklift cage and placed at least one of his feet on the forklift’s dash

board (Figure #5a and 5b). His foot came in contact with and engaged the forklift’s middle control

lever, pushing it in the downward direction. This caused the forklift mast to tilt back towards the forklift

cage, crushing the victim between the mast and the cage.

A janitor passing by saw the victim and notified the office of the incident. A call was placed by

someone in the office for emergency medical services (EMS). Company employees went to assist

the victim and had to push the middle lever up to get the mast to tilt away from the forklift cage. This

freed the victim and the co­workers removed him from the forklift. The local fire department arrived

within minutes of the call and started cardiopulmonary resuscitation (CPR). The victim was then

transported to a local hospital where he was pronounced dead.

**Back to Top**

**Cause of Death**

The medical examiner listed the cause of death as compression asphyxia.

**Recommendations/Discussion**

***Recommendation #1: Employers should ensure that forklift operators never position***

***themselves or any part of their bodies between the forklift operator’s cage and the***

***upright of the mast while the forklift is running.***

**Discussion:**In this case, the forklift was running while the victim was standing partially on the

dashboard and reaching between the forklift’s upright mast and the operator’s cage to see what the

raised load was caught on. While he was standing on the dashboard, his foot had engaged the lever

that controls the tilting of the mast, causing the mast to tilt back towards the operator’s cage, crushing

him.

Forklift operators should never access the area around and between the forklift’s upright masts and

the operator’s cage while the machine is running. This same message is stated in the OSHA

regulation 29 CFR 1910.178,*Powered industrial trucks*, which prohibits the placement of arms or

legs between the uprights of the mast or outside the running lines of the truck.1

***Recommendation #2: Employers should ensure that standard operating procedures***

***(SOP) are followed during forklift operation and that SOPs include alternative***

***procedures for non­routine tasks, such as inability to lower the tines.***

**Discussion:**In this case, the company had previously developed standard operating procedures

(SOP) for forklifts. Employers should ensure that employees follow developed SOPs at all times. This

can be accomplished by performing random inspection of work practices and retraining employees if

it is discovered that all or part of the SOPs are not being followed. SOPs should include alternative

procedures for non­routine situations when employees may have to deviate from the SOP. The

alternative procedures should ensure that the operator and surrounding workers remain safe while

the situation is resolved.

A SOP to exit a forklift typically includes:

1.  Lower the forklift’s tines to the ground.

2.  Set the forklift’s parking brake.

3.  Set the forklift’s travel directional controls to neutral.

4.  Turn off the forklift’s engine.

5.  Block the forklift’s wheels if parked on an incline.

During situations like this, when forklift operators might not be able to lower raised forklift tines, the

operators would not be able to complete the first step of the above standard procedure. Therefore an

alternative procedure for the above SOP would be implemented by the operator. The alternative

procedure would direct the operator to complete steps two through five to ensure the situation is as

safe as possible. Although the potential hazard of a load falling off the raised tines would be present,

if steps two through five are implemented, the forklift’s control levers could not be engaged, even if

someone unintentionally came in contact with them.

***Recommendation #3: Employers should ensure adequate light is provided in locations***

***where forklifts are operated.***

**Discussion:** Although lighting might not have been a contributing factor in this incident, it is possible

that the trailer may have been dimly lit due to only one forklift light working and potential problems

with the dock light. OSHA requires additional directional lighting be provided if the general lighting is

less that two lumens per square foot in any location where forklifts or other powered industrial trucks

will be operated.1 If the light level in an area where forklifts are going to be operated is less than two

lumens per square foot, then employers shall address the hazard by supplying additional lighting,

such as auxiliary directional lighting on the industrial truck.

***Recommendation #4: Employers should ensure that all federal and state required***

***trainings and licenses for forklift operators are up to date.***

**Discussion:**Employers have to comply with federal and state requirements before allowing

employees to operate forklifts.

1) *Federal requirements*: In this case, the employer did have a powered industrial truck training

program that was used to train employees in the operation of forklifts, as required by OSHA. This

federal powered industrial truck training, required for forklift operators, shall be refreshed every three

years. At the time of the incident, more than three years had passed since the victim’s previous forklift

training, although the victim was still performing tasks that involved forklift operation. Employers shall

ensure that their employees’ federal powered industrial truck trainings are refreshed prior to the

three year mark.1 If more than three years pass before the refresher training is provided, employers

should ensure that these employees are assigned tasks that do not require operating forklifts until

they have received the refresher training and evaluation of the training.

2) *Massachusetts requirements*: In Massachusetts, the 1C Hoisting License issued by the

Department of Public Safety (DPS) is required to operate forklifts for work. In order to obtain a

hoisting license, operators must be 18 years of age, complete an application, and successfully pass

an examination covering all working parts of the hoisting machinery, safe operating practices, hand

signals, and inspection procedures.2 Information about the hoisting license can be found on the DPS

Web site at www.mass.gov/dps. In Massachusetts no worker should be operating hoisting

equipment, including forklifts, without a valid Hoisting License.

**Recommendation #5: Employers should routinely review and evaluate the effectiveness of**

**health and safety programs and activities in the workplace.**

**Discussion:** In this case, the employer provided employees with health and safety training, had a

health and safety program, a behavior­based safety program, and a health and safety committee, as

well as standard operating procedures (SOPs) for operating machines and completing tasks. The

company’s health and safety committee included worker representatives and it was reported that the

committee met monthly.

To ensure that health and safety conditions in the workplace improve, employers must ensure that

their health and safety programs and activities are not only implemented and understood, but

routinely evaluated and updated. To ensure that health and safety in workplaces is moving in the

right direction it is important to find routine activities and markers that can help evaluate the overall

effectiveness of health and safety programs and procedures. These activities and markers should

look beyond the absence or reduction in the number of injuries and illnesses. In this case, some

examples of routine activities could include, but not be limited to: 1) monitoring training programs to

ensure that employees’ training and evaluation of the training do not expire before the refresher

trainings are provided; and 2) routinely reviewing all SOPs, including alternative SOPs, to ensure

that they address all hazards associated with incidents, near misses, and non­routine/infrequent but

expected tasks, i.e. freeing a load while operating a powered industrial truck.

In addition, behavior­based safety programs can have the opposite effect of their original intent.

These programs may refocus attention away from identifying and reporting hazards and transfer this

attention on reducing injury reporting, resulting in underreporting of workplace hazards and some

injuries. This will cause a decrease in the number of injuries being reported, but the workplace will

not be safer for the workers. If injuries and near miss incidents are not being reported, then they

cannot be addressed properly. Companies should review their behavior­based safety programs to

ensure they meet the goals of promoting a safer workplace and are encouraging hazards and injury

reporting. OSHA has recently implemented a National Emphasis Program (September 30, 2009) on

underreporting and will review behavior­based safety programs.3 In addition, OSHA has stated that

programs that reward employees for not reporting accidents will be considered a violation of the

OSHA Act 11(c) which prohibits discrimination against employees for participating in health and

safety activities.a

***Recommendation #6: Forklift manufacturers should design forklifts so that operators***

***cannot place any parts of their body in between the cage and mast and unintentionally***

***engage the mast controls.***

**Discussion:** Manufacturers of forklifts should consider addressing this type of crushing hazard and

design forklifts where this hazard is eliminated. There are several devices that would help prevent

the possibility of an operator unintentionally engaging the forklift mast control while positioned

between the mast and cage. Some of these include:

1.  A guard at the front of the operator’s cage designed so a worker could not contact the forklift

controls while in the area between the cage and mast. The guard should be designed so that

it does not impair the operator’s vision and prevents objects from falling back into the

operator’s area.

2.  A safety interlock, requiring forklift operators to engage two controls before moving the forks

and mast.

3.  A pressure interlock within the operator’s seat that would engage by locking the forklift

controls in place when the operator is no longer seated, or a sensor device attached to the

forklift’s seatbelt that when the seatbelt is disconnected the forklift’s power shuts off.


a Description of OSHA 11c requirements www.whistleblowers.gov/index.html. *(Link Updated*

*11/15/2011)*[Report on OSHA’s current policy](http://www.whistleblowersblog.org/2010/05/articles/department-of-labor-1/osha-head-plans-to-improve-whistleblower-program/)

www.whistleblowersblog.org/2010/05/articles/department­of­labor­1/osha­head­plans­to­improve­


whistleblower­program/.

**Figure 1 – Forklift involved in the incident.**

**Figure 2 – Forklift’s controls.**

**Figure 3 – Incident location with a tractor trailer loaded with paper bales not on**

**pallets.**

**Figure 4 – Similar loaded pallet to the one being moved during the incident.**

**Figure 5a – Forklift’s cage and mast.**

**Figure 5b – Diagram of hazard.**

**Back to Top**

**References**

1.  Code of Federal Regulations [1998]. 29 CFR 1910.178. Powered industrial trucks.

Washington, DC: U.S. Printing Office, Office of the Federal Register

2.  Code of Massachusetts Regulations [1999]. 520 CMR 6.00. *Hoisting Machinery.*

3.  OSHA [2009]. Injury and Illness Recordkeeping National Emphasis Program (RK NEP).

USDOL 09­08 (CPL 02), September 30, 2009.

4.  [NIOSH [2001]. NIOSH Alert: preventing injuries and death of workers who operate or work](http://www.cdc.gov/niosh/docs/2001-109/default.html)

[near forklifts, DHHS (NIOSH) Publication No. 2001­109.](http://www.cdc.gov/niosh/docs/2001-109/default.html)

**Back to Top**

**To contact Massachusetts State FACE program personnel regarding State­based FACE**

**reports, please use information listed on the Contact Sheet on the NIOSH FACE web site Please**

**contact In­house FACE program personnel regarding In­house FACE reports and to gain**

**assistance when State­FACE program personnel cannot be reached.**

[Massachusetts Case Reports](http://www2a.cdc.gov/NIOSH-FACE/state.asp?Category=0000&Category2=ALL&State=MA&Submit=Submit)